100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

HEATING & AIR CONDITIONING

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
HEATING & AIR CONDITIONING | 5.3 Condensation lines clog under normal use. | No action required. | Condensation lines will clog under normal conditions. Continued operation of drain line requires Owner maintenance.
| 5.4 Noisy duct work. | Builder will correct oil canning noise if caused by improper installation of duct work. | When metal heats and cools, ticking and cracking may occur. Some creaking will occur due to mechanical connection to floor system and is not covered by this Limited Warranty.
| 5.5 Insufficient heating | Builder will correct if heating system cannot maintain a 70 degree Fahrenheit temperature, under normal operating and weather conditions. Temperature shall be measured at a point 5 ft. above center of floor in affected area. On extremely cold days, a 6 degree difference between actual inside temperature and thermostat setting is acceptable. All rooms may vary in temperature by as much as 4 degrees. | Orientation of the Home, location of rooms and location of vents will also provide a temperature differential. There may be periods when outdoor temperature falls below design temperature thereby lowering temperature in the Home. Certain aspects of the Home including , but not limited to, expansive stairways, open foyers, sunrooms or cathedral ceilings may cause abnormal variation from these Standards and are not covered by this Limited Warranty.
| 5.6 Insufficient cooling. | Builder will correct if cooling system cannot maintain a 78 degree Fahrenheit temperature, under normal operating and weather conditions. Temperature shall be measured at a point 5 ft. above center of the floor in the affected room. On excessively hot days, where outside temperature exceeds 95 degrees Fahrenheit, a difference of 17 degrees from outside temperature will be difficult to maintain. All rooms may vary in temperature by as much as 4 degrees. | Orientation of the Home, location of rooms and location of vents will also provide a temperature differential. There may be periods when outdoor temperature falls below design temperature thereby lowering temperature in the Home. Certain aspects of the Home including , but not limited to, expansive stairways, open foyers, sunrooms or cathedral ceilings may cause abnormal variation from these Standards and are not covered by this Limited Warranty.

Return to Warranty Guidelines Directory

Caring for Your Home Directory