100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

BATHROOMS & KITCHENS

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
BATHROOMS & KITCHENS | 6.1 Cabinet separates from wall | Builder will correct separation in excess of 1/4 inch | Some separation is normal. Caulking is an acceptable method of repair.
| 6.2 Crack in door panel. | Builder will correct only if documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 6.3 Warping of cabinet door or drawer front. | Builder will correct if warp exceeds 3/8 inch as measured from cabinet frame. | Seasonal changes may cause warping and may be a temporary condition.
| 6.4 Doors or drawers do not operate. | Builder will correct. | Owner maintenance is required.
| 6.5 Chips, cracks, scratches on counter top, cabinet fixture, fitting or appliance. | Builder will correct only if documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 6.6 Delamination of counter top or cabinet. | Builder will correct only if documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 6.7 Cracks or chips in fixture. | Builder will correct only if documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 6.8 Defective fixture or appliance. | Builder will correct. | Owner maintenance is required. Appliances are warranted directly through the manufacturer.

Return to Warranty Guidelines Directory

Caring for Your Home Directory