100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

DOORS: INTERIOR

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
DOORS: INTERIOR | 4.1 Latch is loose or rattles. | No action required. | Some minor movement should be expected.
| 4.2 Binds, sticks or does not latch. | Builder will correct one time either at the 45 day list or at the end of one year warranty period. | Seasonal changes may cause doors to expand and contract, and is usually a temporary condition.
| 4.3 Warping. | Builder will correct warping which exceeds 1/4 inch, measured vertically, horizontally or diagonally. | Seasonal changes may cause doors to expand and contract, and are usually temporary conditions.
| 4.4 Excessive opening at bottom. | Builder will correct gaps in excess of 1-1/2 inch between bottom of passage door and finished floor or 2 inch between bottom of closet door and finished floor. | Gaps under doors are intended for air flow.
| 4.5 Rubs on carpet. | Builder will correct. | Builder is not responsible if Owner installs carpet.

Return to Warranty Guidelines Directory

Caring for Your Home Directory