100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

EXTERIOR WALLS

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
EXTERIOR WALLS | 3.20 Entrance of elements through separations of siding or trim joints, or separation between trim and surfaces of masonry or siding. | Builder will correct entrance of elements or separations exceeding 3/8 inch by caulking or other methods. | Any separations 3/8 inch or less are considered routine Owner maintenance.
| 3.21 Cracks in stucco, cement and plaster surfaces. | Builder will correct cracks which exceed 1/8 inch in width. | Hairline cracks are common. Patching and caulking are acceptable methods of repair.
| 3.22 Siding materials deteriorate, delaminate or come loose. | Builder will correct affected area if due to improper workmanship or materials. | Separated, loose or delaminated siding can also be due to improper maintenance. Wavy siding may be due to temperature changes and can be expected.
| 3.23 Paint or stain peels or deteriorates. | Builder will correct. If 75% of a particular wall is affected, entire wall will be corrected. | Some fading is normal and is caused by weathering. Mildew and fungus on siding are caused by climatic conditions and are considered routine maintenance. Varnish or lacquer will deteriorate quickly and is not covered by this Limited Warranty.
| 3.24 Paint splatters and smears on other surfaces. | Builder will correct only if damage is documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 3.25 Faulty application of paint on wall and trim surfaces. | Builder will correct affected area. If greater than 75% of wall or trim piece is affected, entire surface will be corrected. | Some minor imperfections such as over spray, brush marks, etc., are common and should be expected.
| 3.26 Knots bleed through paint or stain. | No action required. | Knots will be apparent and are not considered a defect.
| 3.27 Vent or louver leaks | Builder will correct if caused by improper installation. | Properly installed louvers or vents may at times allow rain or snow to enter under strong wind conditions and is not a deficiency.
| 3.28 Cracks in masonry, veneer, stone, etc. | Builder will correct cracks which exceed 1/4 inch width. | Some cracks are common through masonry and mortar joints. Cracks 1/4 inch or less are considered routine Owner maintenance. Patching is an acceptable method of repair.

Return to Warranty Guidelines Directory

Caring for Your Home Directory