100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

WINDOWS

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
WINDOWS | 3.29 Condensation or frost on interior window surface. | No action required. | Condensation is relative to the quality and type of windows. Temperature differences in high levels of humidity along with individual living habits will cause condensation.
| 3.30 Clouding or condensation between panes of glass. | Builder will correct only if damage is documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 3.31 Glass breakage | Builder will correct only if damage is documented prior to occupancy. | Owner is responsible for establishing a pre-closing walk-through inspection list.
| 3.32 Excessive drafts and leaks. | Builder will correct poorly fitted windows. | Relative to the quality and type of windows, some drafts are normally noticeable around windows, especially during high winds. It may be necessary for the Owner to have storm windows installed to provide a satisfactory solution in high wind areas. All caulking materials expand and contract due to temperature variation and dissimilar materials. Maintenance of weather stripping is Owner's responsibility.
| 3.33 Difficult to open, close or lock. | Builder will correct. | Windows should open, close and lock with reasonable pressure.

Return to Warranty Guidelines Directory

Caring for Your Home Directory