505 1/2 Germantown Pike, Lafayette Hill, PA 19444
800-898-0028

WARRANTY GUILDELINES

ROOFS

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
ROOFS | 3.11 Roof and roof flashing leaks. | Builder will correct if leak occurs under normal conditions. | No action is required if leak is due to snow or ice build-up, high winds or driving rains.
| 3.12 Lifted, torn or curled shingles. | Builder will correct if due to poor installation. | Owner maintenance is required.
| 3.13 Inadequate ventilation. | Builder will provide adequate ventilation. | Moisture accumulation in attics which are not adequately vented is a deficiency. It is the Owner's responsibility to keep existing vents clear of obstructions to promote air flow.
| 3.14 Water stays in gutters. | Builder will correct to limit standing water depth at 1 inch | Owner is responsible for keeping gutters and down spouts clean.
| 3.15 Gutter or down spout leaks. | Builder will correct leaks at connection. | Owner is responsible for keeping gutters and down-spouts clean. Gutters may overflow during heavy rains.

Return to Warranty Guidelines Directory

Caring for Your Home Directory