505 1/2 Germantown Pike, Lafayette Hill, PA 19444
800-898-0028

WARRANTY GUILDELINES

CRAWLSPACES

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
Crawl Spaces | 1.10 Cracks in poured concrete foundation walls. | Builder will correct any crack which exceeds 1\8 in width. | Surface patching and epoxy injection are examples of acceptable repair methods. Shrinkage cracks of 1\8 inch or less are common and should be expected.
| 1.11 Cracks in block or veneer wall. | Builder will correct cracks greater than 1\4 inch in width. | Surface patching and epoxy injection are examples of acceptable repair methods. Shrinkage cracks of 1\4 inch or less are common and should be expected.
| 1.12 Inadequate ventilation. | Builder will install properly sized louvers or vents. | Maintaining adequate ventilation and moisture control, including seasonal adjustment of vent openings, is considered Owner maintenance.
| 1.13 Condensation on walls, joists, support columns and other components of the crawl space area. | No action required. | Maintaining adequate ventilation and moisture control, including seasonal adjustment of vent openings, is considered Owner maintenance.

Return to Warranty Guidelines Directory

Caring for Your Home Directory