100 Springhouse Drive, Suite 105, Collegeville, PA 19426
800-898-0028

WARRANTY GUILDELINES

PLUMBING

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
PLUMBING | 5.7 Refrigerant line leaks. | Builder will correct. | Owner maintenance is required on the system.
| 5.8 Pipe freezes and bursts. | Builder will correct if due to faulty workmanship or materials. | Proper winterization of pipes is considered routine maintenance and Owner should maintain suitable temperature inside the Home.
| 5.9 Noisy water pipe | Builder will correct hammering noise if caused by improper installation. | Some noise can be expected due to flow of water and pipe expansion. This is not a Defect.
| 5.10 Plumbing fixtures, appliances and trim fittings leak or malfunction. | Builder will correct if due to faulty workmanship and materials. | Owner maintenance is required. Scratches, tarnishing or marring must be noted on a pre-closing walk-through inspection list.

Return to Warranty Guidelines Directory

Caring for Your Home Directory