SORRY , SOLD OUT! PLEASE CLICK HERE FOR CURRENT COMMUNITY INFO

Garrison Greene - New Construction Townhomes - Standard Features

INTERIOR DETAILS
9' Ceilings on the first floor on most models Reception foyer with Bruce oak hardwood floor All closets and cased openings fully cased with elegant and easy to care for enameled wood colonial trim detailing Ventilated vinyl coated closet shelving, including the laundry area Distinctive six-panel interior doors Master bedroom suite includes large walk-in closet Plush wall-to-wall Philadelphia brand carpeting in your choice of colors Convenient 2nd floor laundry closets with double doors Easy care no wax flooring in kitchen, powder room, bathrooms and laundry closet Cable TV connection in living room, master bedroom and bonus room Telephone jack in the kitchen, master bedroom and bonus room Clothes washer connection with single lever plumbing hook-up and 220 volt connection to dryer with outside dryer vent
BATHROOM FEATURES
5' One piece fiberglass tub unit in the master and hall baths Aristocraft oak vanities Cultured marble vanity tops Full-width vanity, mirrored medicine cabinet Tub and shower temperature balancing valves Single-lever faucets
KITCHEN FEATURES
Dependable Maytag appliances including a microwave hood and gas stove Food disposal Stainless steel sink with single-lever faucet and spray Easy care Wilsonart or Formica laminate countertops Quality Aristocraft oak cabinets |
EXTERIOR DETAILS
One car garage with detailed entrance and 1/3 h.p. door opener Owens Corning dent resistant vinyl siding Low maintenance soffits & fascia Easy care baked enamel gutters and downspouts Elegant maintenance-free, energy efficient vinyl windows with screens and grilles 25-year architectural fiberglass seal-tab roofing Frost free exterior hose bib located in the garage Underground utilities Public sewer and water Superior two-coat asphalt driveway system Concrete sidewalk from driveway to front door Professionally designed and installed landscaping including grading, seeding, trees and shrubbery, design varies by building and is maintained by the Homeowners Association
QUALITY CONSTRUCTION
3/4" Tongue and groove Sturdifloor plywood floors, glued and nailed Structural strength OSB sheathing on exterior walls Fire suppression sprinkler system Smoke detectors on each floor and in bedrooms Triple hinges on all doors for added strength and alignment 200 amp electrical service Copper water supply lines throughout the house
ENERGY SAVINGS
Insulated 7/8" double pane glass in vinyl windows Special energy efficient inspection program to seal drafts and check air infiltration Insulated steel exterior doors Insulated sliding glass door Economical Carrier high efficiency gas heat furnace with central air conditioning Insulation: R-30 ceilings and R-16 composite walls 50 Gallon electric hot water heater

Garrison Greene Homepage • Adams Model • Barclay Model

Standard Features • Procedures for Buying • Frequently Asked Questions

*** Prices and plans are subject to change and to field variations. ***

Copyright 2001

Michael Anthony Homes
505 1/2 Germantown Pike
Lafayette Hill, PA 19444
800-898-0028