505 1/2 Germantown Pike, Lafayette Hill, PA 19444
800-898-0028

WARRANTY GUILDELINES

DECKS

CATEGORY | OBSERVATION | ACTION REQUIRED BY BUILDER | COMMENTS OR SUGGESTIONS
DECKS | 3.1 Wood twisting, warping or splitting. | Builder will correct only if due to improper installation. | Twisting, warping or splitting of wood deck material is normal due to exposure to the elements. Owner maintenance is required.
| 3.2 Settlement. | Builder will correct slope of deck which exceeds a ratio of 3 inch in a 10 ft. measurement. | Some slope is often provided to allow for water drainage.
| 3.3 Loose railing or post. | Builder will correct if due to improper installation. | Owner maintenance is required.

Return to Warranty Guidelines Directory

Caring for Your Home Directory